**Fenetex Cavity Sizing**

**Geddie Herring**

**Screen My Porch**

**919-605-1738**

**Single Roller**

6” Bracket: 6 x 10

Screen up to 20’

Vinyl up to 16’

7.5” Bracket: 7.5 x 11.5

Screen 20’-25’

Vinyl 16’-25’

**Double Rollers Over / Under**

Two 6” Brackets: 8 x 16

One 6” and One 7.5” Bracket: 9.5 x 17.5

Two 7.5” Brackets: 9.5 x 19

**Double Rollers Side by Side**

Two 6” Brackets: 12 x 10

One 6” and One 7.5” Bracket: 13.5 x 11.5

Two 7.5” Brackets: 15 x 11.5

**Track Recess**

1.75 wide and 2.25 deep (2x and ¾ board)